<http://sourceforge.net/p/brlcad/bugs/311/> ( i logged onto Brl cad and tried to do as stated in the bug report description , i also looked at the images in the bug report description and they weren’t the same )

Create an empty database &Execute screw.tcl (i use the "source" command).

Type: B c\*erase c.r and Render (<http://sourceforge.net/p/brlcad/bugs/270/>).

Went onto mged and tried went into solid edit mode it made a solid and it highlighted more than one. (<http://sourceforge.net/p/brlcad/bugs/197/> )

<http://sourceforge.net/p/brlcad/bugs/180/>

<http://sourceforge.net/p/brlcad/bugs/138/> ( followed link in description and found that it forms a black gap and i looked at the picture presented.