



BRL-CAD to FREECAD

1. Make a model in BRL-CAD and save .g file.
2. Open cmd and change the directory to the bin directory where the BRL-CAD software has been built.
3. Use the g-obj command to change from .g to .obj file. The syntax is as follows:

g-obj <full file name> -o <full output name> <name of geometry to be converted>



1. Open freecad.
2. Make a new document.
3. Click on import in the file tab.
4. Browse and find the .obj file to be imported. Then a dialogue box will appear.
5. Click on Alias Mesh and click on select.



1. The Model will now appear.

