

1.Draw model in MGED

2.Save as database .g



3.open cmd folder where is g-stl and type "g-stl -o name.g name.stl"



4.Open in FreeCAD

5.save as

