


First download and install BRL-CAD

<https://excellmedia.dl.sourceforge.net/project/brlcad/BRL-CAD%20for%20Windows/7.26.0/BRL-CAD_7.26.0.2_x64.exe>


and open it



First command make rec 1 rec for making recange



Similarly using other commands like tec,rpc



At last use rt for making it 3d.

